ORDER FORM

for selection (manufacturing) of dry cooler

Customer (organization name):

1. Required cooling capacity, kW

2. Coolant:

– water

– glycol solution (%)

– other medium (characteristics)

– flow rate, m3/h.

– or kg/h.

– initial temperature, °C:

– end temperature, °C:

3. Ambient air parameters\*:

– temperature, °С:

– relative humidity, %:

\* Ambient air parameters for warm season of the year.

4. Maximum coolant pressure drop, kPa

5. Installation type

horizontal

vertical

V-shaped

6. Dimension limits (if any), m

7. Options:

High temperature protection (“Reversal” configuration)

Protected construction (epoxidation)

Vibration mounts

Automatics set

Fan explosion-proofness

Contact person:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Telephone, fax: